|  |  |  |
| --- | --- | --- |
| **REQUEST FOR QUOTATION (RFQ)** | | Supplier’s Stamp/Signature: |
| Closing Date | : **19 February 2025** |
| Email Submission | : **box3@belts.com.bn** |
| BELTS Ref | : **BELTS/HCCS/RFQ/2025/005** |
| Date of Submission | : Click here to enter text. |
| Supplier/Quote Ref | : Click here to enter text. |

|  |  |
| --- | --- |
| Company Name | **Click here to enter text.** |
| Address | **Click here to enter text.** |
| Phone | Office: **Click here to enter text.** Mobile: **Click here to enter text.** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **No.** | **Item Description** | **Delivery Period** | **Qty/UoM** | **Unit Price** | **Total Price** |
| 1 | **REPLACEMENT OF LIGHT FITTING AT BELTS HQ, LEVEL 5 & 6, SETIA KENANAN OFFICE BLOCK, SETIA KENANGAN COMPLEX, KG. KIULAP.**  **Scope of work:**  To isolate, disconnect and remove existing light fittings. | **2-3 WORKING DAYS UPON PURCHASE ORDER (PO) ISSUANCE** | **1 LOT** | **Click here to enter text.** | **Click here to enter text.** |
| 2 | Supply and install the following replacement light fittings:  **Level 5:**   1. 2 x 18W LED batten fitting 6500K. | **8 SET** | **Click here to enter text.** | **Click here to enter text.** |
| 3 | 1. 3 x 18W LED recessed mirror louvre light fitting 6500K. | **55 SET** | **Click here to enter text.** | **Click here to enter text.** |
| 4 | **Level 6:**   1. 3 x 9W LED recessed mirror louvre light fitting 6500K. | **4 SET** | **Click here to enter text.** | **Click here to enter text.** |
| 5 | 1. 3 x 18W LED recessed mirror louvre light fitting 6500K. | **45 SET** | **Click here to enter text.** | **Click here to enter text.** |
| 6 | 1. 1 x 18W LED batten fitting 6500K | **21 PCS** | **Click here to enter text.** | **Click here to enter text.** |
| 7 | 1. 11W LED 100mm diameter recessed down light 6500K | **86 SET** | **Click here to enter text.** | **Click here to enter text.** |
| 8 | Repair of ceiling caused by light fitting replacement works (where applicable only). | **1 LOT** | **Click here to enter text.** | **Click here to enter text.** |
|  | Note:   * For any site visit purposes kindly e-Mail your date & time schedule to [admincorp@belts.com.bn](mailto:admincorp@belts.com.bn) * For any questions or enquiries kindly e-Mail directly to rfq\_enquiry@belts.com.bn * Contractor must implement safety measures to protect workers and the public during installation/delivery work. * Contractor must complete and submit Risk Assessment and Method Statement (RAMS) to BELTS HSE prior starting work. * Contractor shall comply to SHENA safety requirements and BELTS safety practice. Failure to comply may subject to cessation of work. | | | | |

|  |  |  |
| --- | --- | --- |
| **MANDATORY**  Suppliers are to provide with the Packaging Dimension, Measurement & Weight - in Standard measurement in Meter, Feet, Inches, Cm, Mm, Kg, GM | **TOTAL PRICE** | **Click here to enter text.** |
| Freight Term (EXW,CIF,ETC) | | **Click here to enter text.** |
| Freight Charges (IF APPLICABLE) | | **Click here to enter text.** |
| Any other charges please state | | **Click here to enter text.** |
| **GRAND TOTAL** | | **Click here to enter text.** |

|  |  |
| --- | --- |
| Currency Code : | **BND** |
| Price Validity  (Minimum 9 Months) : | **Click here to enter text.** |
| Payment Terms : | **30 DAYS CREDIT** |
| Warranty : | **Click here to enter text.** |
| Mode of Delivery : | **Click here to enter text.** |
| Delivery Period : | **Click here to enter text.** |
| Country of Manufactured : | **Click here to enter text.** |
| Remarks: | **Click here to enter text.** |